(kicad_sch (version 20210621) (generator eeschema)
  (paper "A5")
  (title_block
    (title "ESP32-C3 minimal")
    (date "2021-09-03")
    (rev "1.0")
    (company "ansemjo")
    (comment 3 "ESP32-C3 module working and program it over USB.")
    (comment 4 "Bare minimal external components to get an")
  )
  (lib_symbols
    (symbol "Connector:USB_B_Micro" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -5.08 11.43 0))
      (property "Value" "USB_B_Micro" (id 1) (at -5.08 8.89 0))
      (property "Footprint" "" (id 2) (at 3.81 -1.27 0))
      (property "Datasheet" "~" (id 3) (at 3.81 -1.27 0))
      (property "ki_keywords" "connector USB micro" (id 4) (at 0 0 0))
      (property "ki_description" "USB Micro Type B connector" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "USB*" (id 6) (at 0 0 0))
      (symbol "USB_B_Micro_0_1"
        (circle (center -3.81 2.159) (radius 0.635) (fill (type outline)))
        (circle (center -0.635 3.429) (radius 0.381) (fill (type outline)))
        (rectangle (start -0.127 -7.62) (end 0.127 -6.858)
          (fill (type none))
        )
        (rectangle (start 5.08 -5.207) (end 4.318 -4.953)
          (fill (type none))
        )
        (rectangle (start 5.08 -2.667) (end 4.318 -2.413)
          (fill (type none))
        )
        (rectangle (start 5.08 -0.127) (end 4.318 0.127)
          (fill (type none))
        )
        (rectangle (start 5.08 4.953) (end 4.318 5.207)
          (fill (type none))
        )
        (rectangle (start 0.254 1.27) (end -0.508 0.508)
          (fill (type outline))
        )
        (rectangle (start -5.08 -7.62) (end 5.08 7.62)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -1.905 2.159)
            (xy 0.635 2.159)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.175 2.159)
            (xy -2.54 2.159)
            (xy -1.27 3.429)
            (xy -0.635 3.429)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.159)
            (xy -1.905 2.159)
            (xy -1.27 0.889)
            (xy 0 0.889)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.699 5.842)
            (xy -4.699 5.588)
            (xy -4.445 4.826)
            (xy -4.445 4.572)
            (xy -1.651 4.572)
            (xy -1.651 4.826)
            (xy -1.397 5.588)
            (xy -1.397 5.842)
            (xy -4.699 5.842)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 2.794)
            (xy 0.635 1.524)
            (xy 1.905 2.159)
            (xy 0.635 2.794)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -4.318 5.588)
            (xy -1.778 5.588)
            (xy -2.032 4.826)
            (xy -4.064 4.826)
            (xy -4.318 5.588)
          )
          (fill (type outline))
        )
      )
      (symbol "USB_B_Micro_1_1"
        (pin power_out line (at 7.62 5.08 180) (length 2.54)
          (name "VBUS")
          (number "1")
        )
        (pin bidirectional line (at 7.62 -2.54 180) (length 2.54)
          (name "D-")
          (number "2")
        )
        (pin bidirectional line (at 7.62 0 180) (length 2.54)
          (name "D+")
          (number "3")
        )
        (pin passive line (at 7.62 -5.08 180) (length 2.54)
          (name "ID")
          (number "4")
        )
        (pin power_out line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "5")
        )
        (pin passive line (at -2.54 -10.16 90) (length 2.54)
          (name "Shield")
          (number "6")
        )
      )
    )
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "C_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "capacitor cap" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0))
      (property "Value" "R_Small" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_Small_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Regulator_Linear:MIC5504-3.3YM5" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 8.89 0))
      (property "Value" "MIC5504-3.3YM5" (id 1) (at -7.62 6.35 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at 0 -10.16 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf" (id 3) (at -6.35 6.35 0))
      (property "ki_keywords" "Micrel LDO voltage regulator" (id 4) (at 0 0 0))
      (property "ki_description" "300mA Low-dropout Voltage Regulator, Vout 3.3V, Vin up to 5.5V, SOT-23" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?23?5*" (id 6) (at 0 0 0))
      (symbol "MIC5504-3.3YM5_0_1"
        (rectangle (start -7.62 -5.08) (end 7.62 5.08)
          (fill (type background))
        )
      )
      (symbol "MIC5504-3.3YM5_1_1"
        (pin power_in line (at -10.16 2.54 0) (length 2.54)
          (name "VIN")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin input line (at -10.16 -2.54 0) (length 2.54)
          (name "EN")
          (number "3")
        )
        (pin no_connect line (at 7.62 -2.54 180) (length 2.54) hide
          (name "NC")
          (number "4")
        )
        (pin power_out line (at 10.16 2.54 180) (length 2.54)
          (name "VOUT")
          (number "5")
        )
      )
    )
    (symbol "local:ESP32-C3-WROOM-02" (in_bom yes) (on_board yes)
      (property "Reference" "U4" (id 0) (at 2.54 37.2406 0))
      (property "Value" "ESP32-C3-WROOM-02" (id 1) (at 12.7 34.4655 0))
      (property "Footprint" "RF_Module:ESP-WROOM-02" (id 2) (at 16.51 -2.54 0))
      (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c3-wroom-02_datasheet_en.pdf" (id 3) (at 53.34 -5.08 0))
      (property "ki_keywords" "RF Radio BT ESP ESP32 C3 Espressif onboard PCB antenna" (id 4) (at 0 0 0))
      (property "ki_description" "RF Module, ESP32-C3 SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, RISC-V, 32-bit, onboard antenna, SMD" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "ESP32?WROOM?32*" (id 6) (at 0 0 0))
      (symbol "ESP32-C3-WROOM-02_0_1"
        (rectangle (start -12.7 33.02) (end 12.7 0)
          (fill (type background))
        )
      )
      (symbol "ESP32-C3-WROOM-02_1_1"
        (pin power_in line (at 0 35.56 270) (length 2.54)
          (name "VDD")
          (number "1")
        )
        (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
          (name "IO10")
          (number "10")
        )
        (pin bidirectional line (at -15.24 7.62 0) (length 2.54)
          (name "RXD/IO20")
          (number "11")
        )
        (pin bidirectional line (at -15.24 10.16 0) (length 2.54)
          (name "TXD/IO21")
          (number "12")
        )
        (pin bidirectional line (at -15.24 16.51 0) (length 2.54)
          (name "D-/IO18")
          (number "13")
        )
        (pin bidirectional line (at -15.24 19.05 0) (length 2.54)
          (name "D+/IO19")
          (number "14")
        )
        (pin bidirectional line (at 15.24 22.86 180) (length 2.54)
          (name "IO3")
          (number "15")
        )
        (pin bidirectional line (at 15.24 25.4 180) (length 2.54)
          (name "IO2")
          (number "16")
        )
        (pin bidirectional line (at 15.24 27.94 180) (length 2.54)
          (name "IO1")
          (number "17")
        )
        (pin bidirectional line (at 15.24 30.48 180) (length 2.54)
          (name "IO0")
          (number "18")
        )
        (pin passive line (at 0 -2.54 90) (length 2.54) hide
          (name "GND")
          (number "19")
        )
        (pin input line (at -15.24 30.48 0) (length 2.54)
          (name "EN")
          (number "2")
        )
        (pin bidirectional line (at 15.24 20.32 180) (length 2.54)
          (name "IO4")
          (number "3")
        )
        (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
          (name "IO5")
          (number "4")
        )
        (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
          (name "IO6")
          (number "5")
        )
        (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
          (name "IO7")
          (number "6")
        )
        (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
          (name "IO8")
          (number "7")
        )
        (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
          (name "IO9")
          (number "8")
        )
        (pin power_in line (at 0 -2.54 90) (length 2.54)
          (name "GND")
          (number "9")
        )
      )
    )
    (symbol "power:+3.3V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3.3V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3.3V\"" (id 5) (at 0 0 0))
      (symbol "+3.3V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3.3V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 67.31 41.91) (diameter 1.016) (color 0 0 0 0))
  (junction (at 73.66 41.91) (diameter 1.016) (color 0 0 0 0))
  (junction (at 99.06 41.91) (diameter 1.016) (color 0 0 0 0))
  (junction (at 125.73 41.91) (diameter 1.016) (color 0 0 0 0))
  (junction (at 133.35 36.83) (diameter 1.016) (color 0 0 0 0))
  (no_connect (at 46.99 76.2))
  (no_connect (at 57.15 71.12))
  (no_connect (at 110.49 74.93))
  (no_connect (at 110.49 77.47))
  (no_connect (at 140.97 54.61))
  (no_connect (at 140.97 57.15))
  (no_connect (at 140.97 62.23))
  (no_connect (at 140.97 64.77))
  (no_connect (at 140.97 67.31))
  (no_connect (at 140.97 69.85))
  (no_connect (at 140.97 72.39))
  (no_connect (at 140.97 80.01))
  (wire (pts (xy 57.15 66.04) (xy 110.49 66.04)))
  (wire (pts (xy 57.15 68.58) (xy 110.49 68.58)))
  (wire (pts (xy 60.96 41.91) (xy 60.96 60.96)))
  (wire (pts (xy 60.96 41.91) (xy 67.31 41.91)))
  (wire (pts (xy 60.96 60.96) (xy 57.15 60.96)))
  (wire (pts (xy 67.31 41.91) (xy 73.66 41.91)))
  (wire (pts (xy 67.31 44.45) (xy 67.31 41.91)))
  (wire (pts (xy 67.31 49.53) (xy 67.31 52.07)))
  (wire (pts (xy 73.66 41.91) (xy 76.2 41.91)))
  (wire (pts (xy 73.66 46.99) (xy 73.66 41.91)))
  (wire (pts (xy 73.66 46.99) (xy 76.2 46.99)))
  (wire (pts (xy 96.52 41.91) (xy 99.06 41.91)))
  (wire (pts (xy 99.06 41.91) (xy 99.06 44.45)))
  (wire (pts (xy 99.06 41.91) (xy 125.73 41.91)))
  (wire (pts (xy 99.06 49.53) (xy 99.06 52.07)))
  (wire (pts (xy 125.73 36.83) (xy 125.73 41.91)))
  (wire (pts (xy 125.73 41.91) (xy 125.73 49.53)))
  (wire (pts (xy 133.35 36.83) (xy 125.73 36.83)))
  (wire (pts (xy 133.35 36.83) (xy 133.35 39.37)))
  (wire (pts (xy 140.97 59.69) (xy 144.78 59.69)))
  (wire (pts (xy 140.97 74.93) (xy 144.78 74.93)))
  (wire (pts (xy 143.51 36.83) (xy 133.35 36.83)))
  (wire (pts (xy 143.51 39.37) (xy 143.51 36.83)))
  (wire (pts (xy 149.86 59.69) (xy 152.4 59.69)))
  (wire (pts (xy 149.86 74.93) (xy 152.4 74.93)))
  (wire (pts (xy 152.4 58.42) (xy 152.4 59.69)))
  (wire (pts (xy 152.4 73.66) (xy 152.4 74.93)))
  (text "This regulator does not meet Espressif's recommendation\nof at least 500mA rating! It's only rated for 300mA.\nWorks for me(tm) but YMMV."
    (at 58.42 33.02 0)
  )
  (text "I used an Ai-Thinker ESP-C3-12F\nmodule but the pinouts are similar."
    (at 130.81 96.52 0)
  )
  (global_label "EN" (shape input) (at 110.49 54.61 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 105.7371 54.5306 0))
  )
  (global_label "BOOTLOADER" (shape input) (at 140.97 77.47 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 155.2782 77.3906 0))
  )
  (symbol (lib_id "power:+5V") (at 73.66 41.91 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR03" (id 0) (at 73.66 45.72 0))
    (property "Value" "+5V" (id 1) (at 71.911 37.465 0))
    (property "Footprint" "" (id 2) (at 73.66 41.91 0))
    (property "Datasheet" "" (id 3) (at 73.66 41.91 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3V") (at 99.06 41.91 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR05" (id 0) (at 99.06 45.72 0))
    (property "Value" "+3.3V" (id 1) (at 99.441 37.5158 0))
    (property "Footprint" "" (id 2) (at 99.06 41.91 0))
    (property "Datasheet" "" (id 3) (at 99.06 41.91 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3V") (at 152.4 58.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR010" (id 0) (at 152.4 62.23 0))
    (property "Value" "+3.3V" (id 1) (at 152.781 54.0258 0))
    (property "Footprint" "" (id 2) (at 152.4 58.42 0))
    (property "Datasheet" "" (id 3) (at 152.4 58.42 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3V") (at 152.4 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR011" (id 0) (at 152.4 77.47 0))
    (property "Value" "+3.3V" (id 1) (at 152.781 69.2658 0))
    (property "Footprint" "" (id 2) (at 152.4 73.66 0))
    (property "Datasheet" "" (id 3) (at 152.4 73.66 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 49.53 76.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR01" (id 0) (at 49.53 82.55 0))
    (property "Value" "GND" (id 1) (at 49.657 80.5942 0))
    (property "Footprint" "" (id 2) (at 49.53 76.2 0))
    (property "Datasheet" "" (id 3) (at 49.53 76.2 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 67.31 52.07 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR02" (id 0) (at 67.31 58.42 0))
    (property "Value" "GND" (id 1) (at 67.437 56.4642 0))
    (property "Footprint" "" (id 2) (at 67.31 52.07 0))
    (property "Datasheet" "" (id 3) (at 67.31 52.07 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 86.36 52.07 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR04" (id 0) (at 86.36 58.42 0))
    (property "Value" "GND" (id 1) (at 86.487 56.4642 0))
    (property "Footprint" "" (id 2) (at 86.36 52.07 0))
    (property "Datasheet" "" (id 3) (at 86.36 52.07 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 99.06 52.07 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR06" (id 0) (at 99.06 58.42 0))
    (property "Value" "GND" (id 1) (at 99.187 56.4642 0))
    (property "Footprint" "" (id 2) (at 99.06 52.07 0))
    (property "Datasheet" "" (id 3) (at 99.06 52.07 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 125.73 87.63 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR07" (id 0) (at 125.73 93.98 0))
    (property "Value" "GND" (id 1) (at 125.857 92.0242 0))
    (property "Footprint" "" (id 2) (at 125.73 87.63 0))
    (property "Datasheet" "" (id 3) (at 125.73 87.63 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 133.35 44.45 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR08" (id 0) (at 133.35 50.8 0))
    (property "Value" "GND" (id 1) (at 133.477 48.8442 0))
    (property "Footprint" "" (id 2) (at 133.35 44.45 0))
    (property "Datasheet" "" (id 3) (at 133.35 44.45 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 143.51 44.45 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR09" (id 0) (at 143.51 50.8 0))
    (property "Value" "GND" (id 1) (at 143.637 48.8442 0))
    (property "Footprint" "" (id 2) (at 143.51 44.45 0))
    (property "Datasheet" "" (id 3) (at 143.51 44.45 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small") (at 147.32 59.69 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R1" (id 0) (at 147.32 54.9868 90))
    (property "Value" "10kΩ" (id 1) (at 147.32 57.7619 90))
    (property "Footprint" "" (id 2) (at 147.32 59.69 0))
    (property "Datasheet" "~" (id 3) (at 147.32 59.69 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 147.32 74.93 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R2" (id 0) (at 147.32 70.2268 90))
    (property "Value" "10kΩ" (id 1) (at 147.32 73.0019 90))
    (property "Footprint" "" (id 2) (at 147.32 74.93 0))
    (property "Datasheet" "~" (id 3) (at 147.32 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 67.31 46.99 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C1" (id 0) (at 69.6342 46.0815 0))
    (property "Value" "1µF" (id 1) (at 69.6342 48.8566 0))
    (property "Footprint" "" (id 2) (at 67.31 46.99 0))
    (property "Datasheet" "~" (id 3) (at 67.31 46.99 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 99.06 46.99 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C2" (id 0) (at 101.3842 46.0815 0))
    (property "Value" "1µF" (id 1) (at 101.3842 48.8566 0))
    (property "Footprint" "" (id 2) (at 99.06 46.99 0))
    (property "Datasheet" "~" (id 3) (at 99.06 46.99 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 133.35 41.91 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C3" (id 0) (at 135.6742 41.0015 0))
    (property "Value" "10µF" (id 1) (at 135.6742 43.7766 0))
    (property "Footprint" "" (id 2) (at 133.35 41.91 0))
    (property "Datasheet" "~" (id 3) (at 133.35 41.91 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 143.51 41.91 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C4" (id 0) (at 145.8342 41.0015 0))
    (property "Value" "100nF" (id 1) (at 145.8342 43.7766 0))
    (property "Footprint" "" (id 2) (at 143.51 41.91 0))
    (property "Datasheet" "~" (id 3) (at 143.51 41.91 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:USB_B_Micro") (at 49.53 66.04 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J1" (id 0) (at 50.927 54.4534 0))
    (property "Value" "USB_B_Micro" (id 1) (at 50.927 57.2285 0))
    (property "Footprint" "" (id 2) (at 53.34 67.31 0))
    (property "Datasheet" "~" (id 3) (at 53.34 67.31 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "Regulator_Linear:MIC5504-3.3YM5") (at 86.36 44.45 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U1" (id 0) (at 86.36 35.4034 0))
    (property "Value" "MIC5504-3.3YM5" (id 1) (at 86.36 38.1785 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at 86.36 54.61 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf" (id 3) (at 80.01 38.1 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "local:ESP32-C3-WROOM-02") (at 125.73 85.09 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U2" (id 0) (at 129.54 87.2194 0))
    (property "Value" "ESP32-C3-WROOM-02" (id 1) (at 139.7 89.9945 0))
    (property "Footprint" "RF_Module:ESP-WROOM-02" (id 2) (at 142.24 87.63 0))
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c3-wroom-02_datasheet_en.pdf" (id 3) (at 179.07 90.17 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR02") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR03") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR04") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR05") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR06") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR07") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR08") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR09") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR010") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR011") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "1µF") (footprint "")
    )
    (path
      (reference "C2") (unit 1) (value "1µF") (footprint "")
    )
    (path
      (reference "C3") (unit 1) (value "10µF") (footprint "")
    )
    (path
      (reference "C4") (unit 1) (value "100nF") (footprint "")
    )
    (path
      (reference "J1") (unit 1) (value "USB_B_Micro") (footprint "")
    )
    (path
      (reference "R1") (unit 1) (value "10kΩ") (footprint "")
    )
    (path
      (reference "R2") (unit 1) (value "10kΩ") (footprint "")
    )
    (path
      (reference "U1") (unit 1) (value "MIC5504-3.3YM5") (footprint "Package_TO_SOT_SMD:SOT-23-5")
    )
    (path
      (reference "U2") (unit 1) (value "ESP32-C3-WROOM-02") (footprint "RF_Module:ESP-WROOM-02")
    )
  )
)
